**Safety Mat Wiring**

**To Connect a Safety Mat to ES500 control, use and Access Automation  
harness # A600-00007-01.**

**Connect the mat to the black and white wires and plug the harness into  
CN6** **on the ES500 control board.**

**The remaining wires are unused.**